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Abstract
This study reported on the preparation of newly low pressure active reverse osmosis (LPARO) membrane by phase inversion technique. The effect of cetyl trimethylammonium bromide (CTAB) and sodium dodecyl sulphate (SDS) as surfactants on performance and morphological structure were examined. Using brackish water as a sample, the membrane performance was evaluated in terms of pure water permeation (PWP), flux and salt rejection. Experimental data revealed that at 2.0 wt. % of SDS, the LPARO membrane achieved the optimum performance and produced the finest membrane.
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Abstrak
Kajian ini melaporkan mengenai penyediaan membran osmosis songsang aktif bertekanan rendah (LPARO) dengan teknik fasa penyongsangan. Kesan setil trimetilammonium bromida (CTAB) dan natrium dodekil sulfat (SDS) sebagai surfaktan terhadap prestasi dan struktur morfologi telah diselidik. Dengan menggunakan air payau sebagai contoh, prestasi membran telah dinilai dari segi penyerapan air tulen (PWP),  penyingkiran fluks dan garam.  Data  eksperimen  menunjukkan bahawa pada 2.0 wt . % SDS, membran LPARO berjaya mencapai prestasi yang optimum dan menghasilkan membran yang terbaik.
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