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Abstract
Manganese oxide (Mn2O3) mesoporous carbon (MPC) was synthesized by the incipient wetness of impregnation at room temperature and followed by calcination of 300 °C. The structure and morphology of Mn2O3/MPC were characterized by Fourier transform infrared (FTIR) spectrum, atomic force microscopy (AFM) and field emission scanning electron microscopy (FESEM). The electrochemical performance of synthesized composites was evaluated by cyclic voltammetry (CV), galvanostatic measurement of charge-discharge (GCD) as well as power and energy density characteristics. The specific capacitance of the composite electrode when 10 wt.% Mn salt was coated on the surface of MPC film could reach 53.59 mF cm-2 as compared to MPC film at only 15.23 mF cm-2. These are in good agreement with the electrochemical performance improvement results of the energy and power density recorded for Mn2O3/MPC, which lead to higher specific capacitance as supported by the CV and GCD results in 1 M potassium chloride (KCl) of electrolyte. This enhanced capacitance was attributed to the outstanding electric properties of MPC film as well as the faradaic redox reactions of manganese oxide as proven by FESEM and EDX analysis. The results indicate the promising application of the fabricated Mn2O3/MPC composite as electrodes for supercapacitors.
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Abstrak
[bookmark: _Hlk26568203]Mangan oksida (Mn2O3) karbon filem berliang meso (MPC) telah disintesis melalui kaedah serapan basah pada suhu bilik dan diikuti oleh proses pengkalsinan pada suhu 300 °C. Struktur dan morfologi Mn2O3/MPC dicirikan oleh spektrum inframerah transformasi Fourier (FTIR), mikroskop kekuatan atom (AFM) dan mikroskop pengimbasan elektron serta pelepasan medan (FESEM). Prestasi elektrokimia komposit yang disintesis telah dinilai oleh kitaran voltammetri (CV), pengukuran pelepasan galvanostatik (GCD) juga ciri-ciri kuasa dan ketumpatan tenaga. Kapasitan khusus elektrod komposit apabila garam 10 wt.% Mn dilapisi pada permukaan MPC filem boleh mencapai 53.59 mF cm-2 berbanding dengan MPC filem hanya 15.23 mF cm-2. Ini menyamai dengan peningkatan prestasi elektrokimia terhadap tenaga dan ketumpatan kuasa yang dicatatkan untuk Mn2O3/MPC, yang membawa kepada kapasitan khusus yang lebih tinggi, disokong oleh keputusan CV dan GCD dalam elektrolit 1 M kalium klorida (KCl). Peningkatan kapasitan ini adalah disebabkan oleh sifat-sifat elektrik yang cemerlang dari MPC filem serta tindak balas redoks faradaik dari mangan seperti yang dibuktikan juga dalam analisis FESEM dan EDX. Keputusan menunjukkan fabrikasi komposit Mn2O3/MPC mempunyai potensi aplikasi sebagai elektrod bagi superkapasitor.

Kata kunci:  mangan oksida, karbon berliang meso, komposit, kapasitan khusus, superkapasitor
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